[bookmark: _GoBack]DAE    = STANDARD LOGGING by means of the internal memory (eeprom)
* General details from the charger
- Charge setting
- Charger model
- Total number of started charging processes
- Total number of finished charging processes (LED green)
- Total number of times that the temperature protection was initiated 
- Total number of times charge that the time monitoring was initiated
- Total number of times the charge current was reduced
- Total number of times the battery was discharged too deeply 
- Total number of times the battery voltage was too high

* Registers extensive details from the last two charging processes
Above information can be copied from the internal memory to a SD card.


DAL 	= EXTENSIVE LOGGING by means of a pre-inserted SD card
* All information from the standard DAE logging
* All details from every single charging process
* The course of every single charging process can be displayed in a diagram
* One easy table shows for every single charging process: 
- charge process finished yes/no
- which errors occurred
- how much Ah is charged into the battery


